CSCI 355 Lab Manual. Copyright © 1999, P. Walsh, Malaspina University College. 40

Appendix A (Data Sheets)

Note, a, b, c, d, e, f, g and dp are active low and MUST be grounded through a resistor. For this task, use an R470 resistor IC. It is a 16 pin IC containing 8 resistors. Assume the normal IC orientation and pin labeling. The following pin pairs specify the the I/O pins for the 8 resistors: (P1, P16), (P2, P15) (P3, P14), (P4, P13), (P5, P12), (P6, P11), (P7, P10), (P8, P9).